**Uniden Bearcat BCD996P2**

**Software**

[ARC XT BASIC version 2.0 build 6](http://www.butel.nl/download/arcxt/arcxt_setup20.zip) <http://www.butel.nl/download_xt.html>

Serial Drivers for USB <http://info.uniden.com/UnidenMan4/BCD996P2>

**Programming Elements**

**Conventional System/Trunk Site** - (only 1 trunked site per system), (assign quick key to each)

**Groups** - (assign quick key to each)

**Channels**

**Frequencies or ID’s** - Conventional Site or Trunk Site)

**Start-Up Keys: (0-9) - Conventional System, Trunk Site**

Quick Keys: (0-99) - Conventional System, Trunk Site, Trunk Group

Number Tags: (0-999) - Systems, Channels

**UCAN = Top of Utah Public Service Repeaters**

**START-UP KEYS (press/hold key while turning on radio)**

**0 = Scan Conventional (UCAN + Ham & Airports)**

**1 = UCAN Site Trunked >>> Mt Ogden**

**2 = UCAN Site Trunked >>> Weber Co**

**3 = UCAN Site Trunked >>> Promontory**

**4 = UCAN Site Trunked >>> Davis Co**

**5 = UCAN Site Trunked >>> Francis Peak**

**6 = UCAN Site Trunked >>> Layton**

**7 =Scan Ham Radio (no UCAN) - 2 meters and 70 centimeters) & Airports**